**Department of Infrastructure and Transport**

**Vehicle Safety Operations Branch**

**Road-Friendly Suspension Certificate Number (RFCN): RF2037**

 **Issue Date: 2 July 2025**

The Director, Technical Assessment and Approvals, TAA, has assessed the information in Schedule 3

for the suspension described in this Road Friendly Certificate, which the Supplier identified in

Schedule 1 has submitted, as complying with the road-friendliness requirements as specified in

NTC publication ‘Road-Friendly Suspension – Performance and Component Requirements, and

Acceptable Test Methods’. This information will be acceptable for use as evidence of compliance

with the requirements specified in the above NTC publication. Provided the suspension is installed

according to the Supplier’s nominated installation instructions identified in Schedule 3.

The issue of this Certificate is subject to the following conditions:

1. The Supplier shall not quote the Road-Friendly Certificate Number in respect of a suspension which is not the suspension certified in the Road–Friendly Suspension certificate with that number.

1. Without the prior approval of the General Manager, Vehicle Safety Standards Branch, the Supplier shall not quote Road-Friendly Certificate Number in respect of a suspension, that is in any way different from the suspension described in the final form of the application for this Suspension Certificate Number. The application includes reports and other information relating to the application.
2. The Supplier shall by detailed quality control and test ensure continuing compliance with the requirements.
3. The Supplier shall maintain records of detailed quality control and test documentation.
4. The Supplier shall supply upon request, to General Manager, Vehicle Safety Standards Branch any additional information requested for the purpose of demonstrating compliance.
5. The Supplier shall not quote the Road-Friendly Certificate Number in respect of a suspension on or after the Expiry date specified in the certificate.
6. The Supplier shall indicate by an appropriate method (decal, label or plate) the Road-Friendly Suspension Certificate Number (RFCN) on the suspension system, or on a suitable location on the vehicle near the installed suspension or the vehicle compliance plate.
7. On cessation of marketing the specified suspension in Australia, the Supplier shall notify General Manager, Vehicle Safety Standards Branch of the date of manufacture of the last specified suspension supplied to the market in Australia.
8. If the requirements for road-friendliness are changed by the National Road Transport Commission, a new approval may be required.

Certificate No: **RF2037**

### 1st Issue Date: **30 October 2012**

Expiry Date: **Life of Model**

# SCHEDULE 1

**Supplier Name**: Fuwa K Hitch (Australia) Pty Ltd **Supplier ID**:

**Supplier Address**: 13-21 Bliss Court
DERRIMUT VIC 3030

# SCHEDULE 2

**Make:** K-HITCH

**Model:** KHAS

# SCHEDULE 3

|  |  |  |  |
| --- | --- | --- | --- |
|  | Variant 1 | Variant 2 | Variant 3 |
| Variant name: | KHAS-9-OS-F1-300 | KHAS-9-OS-F1-350 | KHAS-22-US-F1-300 |
| Number of Axles | 1 | 1 | 1 |
| Overslung/Underslung | O/SLUNG | O/SLUNG | U/SLUNG |
| Maximum Axle spread (m) | 0.000 | 0.000 | 0.000 |
| Dampers Part Numbers | KHAS 075 | KHAS 075 | KHAS 075 |
| Smallest Tyre Size Designation | 8.25R15 | 8.25R15 | 8.25R15 |
| Highest tyre pressure (Kpa) | 825 | 825 | 825 |
| Airbag Diameter (mm) | 300 | 350 | 300 |
| Reference Drawings No of Suspension (parts list & assembly details) | KHAS 060-380F1KHAS 060-405F1KHAS 060 430F1 | KHAS 060-380F1KHAS 060-405F1KHAS 060 430F1 | KHAS 055-250F1KHAS 055-300F1 |

|  |  |  |  |
| --- | --- | --- | --- |
|  | Variant 4 | Variant 5 | Variant 6 |
| Variant name: | KHAS-11-US-F1-350 | KHAS-9-US-F1-300 | KHAS-9-US-F1-350 |
| Number of Axles | 1 | 1 | 1 |
| Overslung/Underslung | U/SLUNG | U/SLUNG | O/SLUNG |
| Maximum Axle spread (m) | 0.000 | 0.000 | 0.000 |
| Dampers Part Numbers | KHAS 075 | KHAS 075 | KHAS 075 |
| Smallest Tyre Size Designation | 8.25R15 | 8.25R15 | 8.25R15 |
| Highest tyre pressure (Kpa) | 825 | 825 | 825 |
| Airbag Diameter (mm) | 350 | 300 | 350 |
| Reference Drawings No of Suspension (parts list & assembly details) | KHAS 055-250F1KHAS 055-300F1 | KHAS 060-380F1KHAS 060-405F1KHAS 060 430F1 | KHAS 060-380F1KHAS 060-405F1KHAS 060 430F1 |

|  |  |  |  |
| --- | --- | --- | --- |
|  | Variant 7 | Variant 8 | Variant 9 |
| Variant name: | KHAS-11-OS-F1-300 | KHAS-11-OS-F1-350 | KHAS-9-OS-R1-300 |
| Number of Axles | 1 | 1 | 1 |
| Overslung/Underslung | O/SLUNG | O/SLUNG | O/SLUNG |
| Maximum Axle spread (m) | 0.000 | 0.000 | 0.000 |
| Dampers Part Numbers | KHAS 075 | KHAS 075 | KHAS 071KKHAS 071P |
| Smallest Tyre Size Designation | 8.25R15 | 8.25R15 | 8.25R15 |
| Highest tyre pressure (Kpa) | 825 | 825 | 825 |
| Airbag Diameter (mm) | 300 | 350 | 300 |
| Reference Drawings No of Suspension (parts list & assembly details) | KHAS 055-250F1KHAS 055-300F1 | KHAS 055-250F1KHAS 055-300F1 | KHAS 060-380R1KHAS 060-405R1KHAS 060 430R1 |

|  |  |  |  |
| --- | --- | --- | --- |
|  | Variant 10 | Variant 11 | Variant 12 |
| Variant name: | KHAS-9-OS-R1-350 | KHAS-11-US-R1-300 | KHAS-11-US-R1-350 |
| Number of Axles | 1 | 1 | 1 |
| Overslung/Underslung | O/SLUNG | U/SLUNG | U/SLUNG |
| Maximum Axle spread (m) | 0.000 | 0.000 | 0.000 |
| Dampers Part Numbers | KHAS 071KKHAS 071P | KHAS 071KKHAS 071P | KHAS 071KKHAS 071P |
| Smallest Tyre Size Designation | 8.25R15 | 8.25R15 | 8.25R15 |
| Highest tyre pressure (Kpa) | 825 | 825 | 825 |
| Airbag Diameter (mm) | 350 | 300 | 350 |
| Reference Drawings No of Suspension (parts list & assembly details) | KHAS 060-380R1KHAS 060-405R1KHAS 060 430R1 | KHAS 055-250R1KHAS 055-300R1 | KHAS 055-250R1KHAS 055-300R1 |

|  |  |  |  |
| --- | --- | --- | --- |
|  | Variant 13 | Variant 14 | Variant 15 |
| Variant name: | KHAS-9-US-R1-300 | KHAS-9-US-R1-350 | KHAS-11-OS-R1-300 |
| Number of Axles | 1 | 1 | 1 |
| Overslung/Underslung | U/SLUNG | U/SLUNG | O/SLUNG |
| Maximum Axle spread (m) | 0.000 | 0.000 | 0.000 |
| Dampers Part Numbers | KHAS 071KKHAS 071P | KHAS 071KKHAS 071P | KHAS 071KKHAS 071P |
| Smallest Tyre Size Designation | 8.25R15 | 8.25R15 | 8.25R15 |
| Highest tyre pressure (Kpa) | 825 | 825 | 825 |
| Airbag Diameter (mm) | 300 | 350 | 300 |
| Reference Drawings No of Suspension (parts list & assembly details) | KHAS 060-380R1KHAS 060-405R1KHAS 060 430R1 | KHAS 060-380R1KHAS 060-405R1KHAS 060 430R1 | KHAS 055-250R1KHAS 055-300R1 |

|  |  |  |  |
| --- | --- | --- | --- |
|  | Variant 16 | Variant 17 | Variant 18 |
| Variant name: | KHAS-11-OS-R1-350 | KHAS-9-OS-F2-300 | KHAS-9-OS-F2-350 |
| Number of Axles | 1 | 2 | 2 |
| Overslung/Underslung | O/SLUNG | O/SLUNG | O/SLUNG |
| Maximum Axle spread (m) | 0.000 | 1.000 | 1.000 |
| Dampers Part Numbers | KHAS 071KKHAS 071P | KHAS 075 | KHAS |
| Smallest Tyre Size Designation | 8.25R15 | 8.25R15 | 8.25R15 |
| Highest tyre pressure (Kpa) | 825 | 825 | 825 |
| Airbag Diameter (mm) | 350 | 300 | 350 |
| Reference Drawings No of Suspension (parts list & assembly details) | KHAS 055-250R1KHAS 055-300R1 | KHAS 060-380F1KHAS 060-405F1KHAS 060 430F1 | KHAS 060-380F1KHAS 060-405F1KHAS 060 430F1 |

|  |  |  |  |
| --- | --- | --- | --- |
|  | Variant 19 | Variant 20 | Variant 21 |
| Variant name: | KHAS-11-US-F2-300 | KHAS-11-US-F2-350 | KHAS-9-US-F2-300 |
| Number of Axles | 2 | 2 | 2 |
| Overslung/Underslung | U/SLUNG | U/SLUNG | U/SLUNG |
| Maximum Axle spread (m) | 1.000 | 1.000 | 2.000 |
| Dampers Part Numbers | KHAS 075 | KHAS 075 | KHAS 075 |
| Smallest Tyre Size Designation | 8.25R15 | 8.25R15 | 8.25R15 |
| Highest tyre pressure (Kpa) | 825 | 825 | 825 |
| Airbag Diameter (mm) | 300 | 350 | 300 |
| Reference Drawings No of Suspension (parts list & assembly details) | KHAS 055-250F1KHAS 055-300F1 | KHAS 055-250F1KHAS 055-300F1 | KHAS 060-380F1KHAS 060-405F1KHAS 060 430F1 |

|  |  |  |  |
| --- | --- | --- | --- |
|  | Variant 22 | Variant 23 | Variant 24 |
| Variant name: | KHAS-9-US-F2-350 | KHAS-11-OS-F2-300 | KHAS-11-OS-F2-350 |
| Number of Axles | 2 | 2 | 2 |
| Overslung/Underslung | U/SLUNG | O/SLUNG | O/SLUNG |
| Maximum Axle spread (m) | 2.000 | 2.000 | 2.000 |
| Dampers Part Numbers | KHAS 075 | KHAS 075 | KHAS 075 |
| Smallest Tyre Size Designation | 8.25R15 | 8.25R15 | 8.25R15 |
| Highest tyre pressure (Kpa) | 825 | 825 | 825 |
| Airbag Diameter (mm) | 350 | 300 | 350 |
| Reference Drawings No of Suspension (parts list & assembly details) | KHAS 060-380F1KHAS 060-405F1KHAS 060 430F1 | KHAS 055-250F1KHAS 055-300F1 | KHAS 055-250F1KHAS 055-300F1 |

|  |  |  |  |
| --- | --- | --- | --- |
|  | Variant 25 | Variant 26 | Variant 27 |
| Variant name: | KHAS-9-OS-F2-300 | KHAS-9-OS-R2-350 | KHAS-11-US-R2-300 |
| Number of Axles | 2 | 2 | 2 |
| Overslung/Underslung | O/SLUNG | O/SLUNG | U/SLUNG |
| Maximum Axle spread (m) | 2.000 | 2.000 | 2.000 |
| Dampers Part Numbers | KHAS 071KKHAS 071P | KHAS 071KKHAS 071P | KHAS 071KKHAS 071P |
| Smallest Tyre Size Designation | 8.25R15 | 8.25R15 | 8.25R15 |
| Highest tyre pressure (Kpa) | 825 | 825 | 825 |
| Airbag Diameter (mm) | 300 | 350 | 300 |
| Reference Drawings No of Suspension (parts list & assembly details) | KHAS 060-380F1KHAS 060-405F1KHAS 060 430F1 | KHAS 060-380F1KHAS 060-405F1KHAS 060 430F1 | KHAS 055-250R1KHAS 055-300R1 |

|  |  |  |  |
| --- | --- | --- | --- |
|  | Variant 28 | Variant 29 | Variant 30 |
| Variant name: | KHAS-11-US-R2-350 | KHAS-9US-R2-300 | KHAS-9-US-R2-350 |
| Number of Axles | 2 | 2 | 2 |
| Overslung/Underslung | U/SLUNG | U/SLUNG | U/SLUNG |
| Maximum Axle spread (m) | 2.000 | 2.000 | 2.000 |
| Dampers Part Numbers | KHAS 071KKHAS 071P | KHAS 071KKHAS 071P | KHAS 071KKHAS 071P |
| Smallest Tyre Size Designation | 8.25R15 | 8.25R15 | 8.25R15 |
| Highest tyre pressure (Kpa) | 825 | 825 | 825 |
| Airbag Diameter (mm) | 350 | 300 | 350 |
| Reference Drawings No of Suspension (parts list & assembly details) | KHAS 055-250R1KHAS 055-300R1 | KHAS 060-380F1KHAS 060-405F1KHAS 060 430F1 | KHAS 060-380F1KHAS 060-405F1KHAS 060 430F1 |

|  |  |  |  |
| --- | --- | --- | --- |
|  | Variant 31 | Variant 32 | Variant 33 |
| Variant name: | KHAS-11-OS-R2-300 | KHAS-11-OS-R2-350 | Khas-9-OS-F3-300 |
| Number of Axles | 2 | 2 | 3 |
| Overslung/Underslung | O/SLUNG | O/SLUNG | O/SLUNG |
| Maximum Axle spread (m) | 2.000 | 2.000 | 3.2000 |
| Dampers Part Numbers | KHAS 071KKHAS 071P | KHAS 071KKHAS 071P | KHAS 075 |
| Smallest Tyre Size Designation | 8.25R15 | 8.25R15 | 8.25R15 |
| Highest tyre pressure (Kpa) | 825 | 825 | 825 |
| Airbag Diameter (mm) | 300 | 350 | 300 |
| Reference Drawings No of Suspension (parts list & assembly details) | KHAS 055-250R1KHAS 055-300R1 | KHAS 055-250R1KHAS 055-300R1 | KHAS 060-380F1KHAS 060-405F1KHAS 060 430F1 |

|  |  |  |  |
| --- | --- | --- | --- |
|  | Variant 34 | Variant 35 | Variant 36 |
| Variant name: | KHAS-9-OS-F3-350 | KHAS-11-US-F3-300 | KHAS-11-US-F3-350 |
| Number of Axles | 3 | 3 | 3 |
| Overslung/Underslung | O/SLUNG | U/SLUNG | U/SLUNG |
| Maximum Axle spread (m) | 3.2000 | 3.2000 | 3.2000 |
| Dampers Part Numbers | KHAS 075 | KHAS 075 | KHAS 075 |
| Smallest Tyre Size Designation | 8.25R15 | 8.25R15 | 8.25R15 |
| Highest tyre pressure (Kpa) | 825 | 825 | 825 |
| Airbag Diameter (mm) | 350 | 300 | 350 |
| Reference Drawings No of Suspension (parts list & assembly details) | KHAS 060-380F1KHAS 060-405F1KHAS 060 430F1 | KHAS 055-250R1KHAS 055-300R1 | KHAS 055-250R1KHAS 055-300R1 |

|  |  |  |  |
| --- | --- | --- | --- |
|  | Variant 37  | Variant 38 | Variant 39 |
| Variant name: | KHAS-9-US-F3-300 | KHAS-9-US-F3-350 | KHAS-11-OS-F3-300 |
| Number of Axles | 3 | 3 | 3 |
| Overslung/Underslung | U/SLUNG | U/SLUNG | O/SLUNG |
| Maximum Axle spread (m) | 3.2000 | 3.2000 | 3.2000 |
| Dampers Part Numbers | KHAS 075 | KHAS 075 | KHAS 075 |
| Smallest Tyre Size Designation | 8.25R15 | 8.25R15 | 8.25R15 |
| Highest tyre pressure (Kpa) | 825 | 825 | 825 |
| Airbag Diameter (mm) | 300 | 350 | 300 |
| Reference Drawings No of Suspension (parts list & assembly details) | KHAS 060-380F1KHAS 060-405F1KHAS 060 430F1 | KHAS 060-380F1KHAS 060-405F1KHAS 060 430F1 | KHAS 055-250R1KHAS 055-300R1 |

|  |  |  |  |
| --- | --- | --- | --- |
|  | Variant 40 | Variant 41 | Variant 42 |
| Variant name: | KHAS-11-OS-F3-350 | KHAS-9-OS-R3-300 | KHAS-9-OS-R3-350 |
| Number of Axles | 3 | 3 | 3 |
| Overslung/Underslung | O/SLUNG | O/SLUNG | U/SLUNG |
| Maximum Axle spread (m) | 3.2000 | 3.2000 | 3.2000 |
| Dampers Part Numbers | KHAS 075 | KHAS 071KKHAS 071P | KHAS 071KKHAS 071P |
| Smallest Tyre Size Designation | 8.25R15 | 8.25R15 | 8.25R15 |
| Highest tyre pressure (Kpa) | 825 | 825 | 825 |
| Airbag Diameter (mm) | 350 | 300 | 350 |
| Reference Drawings No of Suspension (parts list & assembly details) | KHAS 055-250R1KHAS 055-300R1 | KHAS 060-380F1KHAS 060-405F1KHAS 060 430F1 | KHAS 060-380F1KHAS 060-405F1KHAS 060 430F1 |

|  |  |  |  |
| --- | --- | --- | --- |
|  | Variant 43 | Variant 44 | Variant 45 |
| Variant name: | KHAS-11-US-R3-300 | KHAS-11-US-R3-350 | KHAS-9-US-R3-300 |
| Number of Axles | 3 | 3 | 3 |
| Overslung/Underslung | U/SLUNG | U/SLUNG | U/SLUNG |
| Maximum Axle spread (m) | 3.2000 | 3.2000 | 3.2000 |
| Dampers Part Numbers | KHAS 071KKHAS 071P | KHAS 071KKHAS 071P | KHAS 071KKHAS 071P |
| Smallest Tyre Size Designation | 8.25R15 | 8.25R15 | 8.25R15 |
| Highest tyre pressure (Kpa) | 825 | 825 | 825 |
| Airbag Diameter (mm) | 300 | 350 | 300 |
| Reference Drawings No of Suspension (parts list & assembly details) | KHAS 055-250R1KHAS 055-300R1 | KHAS 055-250R1KHAS 055-300R1 | KHAS 060-380F1KHAS 060-405F1KHAS 060 430F1 |

|  |  |  |  |
| --- | --- | --- | --- |
|  | Variant 46 | Variant 47 | Variant 48 |
| Variant name: | KHAS-9-US-R3-350 | KHAS-11-OS-R3-300 | KHAS-11-OS-R3-350 |
| Number of Axles | 3 | 3 | 3 |
| Overslung/Underslung | U/SLUNG | O/SLUNG | O/SLUNG |
| Maximum Axle spread (m) | 3.2000 | 3.2000 | 3.2000 |
| Dampers Part Numbers | KHAS 071KKHAS 071P | KHAS 071KKHAS 071P | KHAS 071KKHAS 071P |
| Smallest Tyre Size Designation | 8.25R15 | 8.25R15 | 8.25R15 |
| Highest tyre pressure (Kpa) | 825 | 825 | 825 |
| Airbag Diameter (mm) | 350 | 300 | 350 |
| Reference Drawings No of Suspension (parts list & assembly details) | KHAS 060-380F1KHAS 060-405F1KHAS 060 430F1 | KHAS 055-250R1KHAS 055-300R1 | KHAS 055-250R1KHAS 055-300R1 |

|  |  |  |  |
| --- | --- | --- | --- |
|  | Variant 49 | Variant 50 | Variant 51 |
| Variant name: | TA-250U-3 | TA-250T-3 | TI-250T-3 |
| Number of Axles | 3 | 3 | 3 |
| Overslung/Underslung | U/SLUNG | O/SLUNG | O/SLUNG |
| Maximum Axle spread (m) | 3.200 | 3.200 | 3.200 |
| Dampers Part Numbers | WCTA001, WCTA002 | WCTA001, WCTA002 | WCTI002 |
| Smallest Tyre Size Designation | 8.25R15 | 8.25R15 | 8.25R15 |
| Highest tyre pressure (Kpa) | 825 | 825 | 825 |
| Airbag Diameter (mm) | 320 | 348 | 830 |
| Reference Drawings No of Suspension (parts list & assembly details) | 120430, 120433, 120434, 120435 | 120228, 120230 | 120409 |

|  |  |  |  |
| --- | --- | --- | --- |
|  | Variant 52 | Variant 53 | Variant 54 |
| Variant name: | TI-250U-3 | TA-250U-2 | TA250T-2 |
| Number of Axles | 3 | 2 | 2 |
| Overslung/Underslung | U/SLUNG | U/SLUNG | O/SLUNG |
| Maximum Axle spread (m) | 3.200 | 2.000 | 2.000 |
| Dampers Part Numbers | WCTI002 WCTA001 WCTA002 | WCTA001, WCTA002 | WCTA001, WCTA002 |
| Smallest Tyre Size Designation | 8.25R15 | 8.25R15 | 8.25R15 |
| Highest tyre pressure (Kpa) | 825 | 825 | 825 |
| Airbag Diameter (mm) | 320 | 320 | 348 |
| Reference Drawings No of Suspension (parts list & assembly details) | 120506 | 120430, 120433, 120434, 120435 | 120228, 120230 |

|  |  |  |  |
| --- | --- | --- | --- |
|  | Variant 55 | Variant 56 | Variant 57 |
| Variant name: | TI-250T-2 | TI250U-2 | TA-250T-1 |
| Number of Axles | 2 | 2 | 1 |
| Overslung/Underslung | O/SLUNG | U/SLUNG | O/SLUNG |
| Maximum Axle spread (m) | 2.000 | 2.000 | 0.000 |
| Dampers Part Numbers | WCTI002 | WCTA001, WCTA002 | WCTA001, WCTA002 |
| Smallest Tyre Size Designation | 8.25R15 | 8.25R15 | 8.25R15 |
| Highest tyre pressure (Kpa) | 825 | 825 | 825 |
| Airbag Diameter (mm) | 380 | 320 | 348 |
| Reference Drawings No of Suspension (parts list & assembly details) | 120409 | 120506 | 120228, 120230 |

|  |  |  |  |
| --- | --- | --- | --- |
|  | Variant 58 | Variant 59 | Variant 60 |
| Variant name: | KT-250U-3 | KT-250U-3 | KT-250U-2 |
| Number of Axles | 3 | 3 | 2 |
| Overslung/Underslung | Underslung | Overslung | Underslung |
| Maximum Axle spread (m) | 3.200 | 3.200 | 2.000 |
| Dampers Part Numbers | WCTA004 | WCTA004 | WCTA004 |
| Smallest Tyre Size Designation | 8.25R15 | 8.25R15 | 8.25R15 |
| Highest tyre pressure (Kpa) | 825 | 825 | 825 |
| Airbag Diameter (mm) | 323 | 348 | 323 |
| Reference Drawings No of Suspension (parts list & assembly details) | N100523, N100552, N100524, N100544, N100545, N100525, N100551, N100543 | N100539, N100526, N100537, N100527, N100540, N100541 | N100523, N100552, N100524, N100544, N100545, N100525, N100551, N100543 |

|  |  |  |  |
| --- | --- | --- | --- |
|  | Variant 61 | Variant 62 | Variant 63 |
| Variant name: | KT-250U-2 | KT-250U-1 | KT-250U-1 |
| Number of Axles | 2 | 1 | 1 |
| Overslung/Underslung | Overslung | Underslung | Overslung |
| Maximum Axle spread (m) | 2.000 | 0.000 | 0.000 |
| Dampers Part Numbers | WCTA004 | WCTA004 | WCTA004 |
| Smallest Tyre Size Designation | 8.25R15 | 8.25R15 | 8.25R15 |
| Highest tyre pressure (Kpa) | 825 | 825 | 825 |
| Airbag Diameter (mm) | 348 | 323 | 348 |
| Reference Drawings No of Suspension (parts list & assembly details) | N100539, N100526, N100537, N100527, N100540, N100541 | N100523, N100552, N100524, N100544, N100545, N100525, N100551, N100543 | N100539, N100526, N100537, N100527, N100540, N100541 |

|  |  |  |  |
| --- | --- | --- | --- |
|  | Variant 64 | Variant 65 | Variant 66 |
| Variant name: | MBS-100-1 | MBS-200-1 | MBS-100-2 |
| Number of Axles | 1 | 1 | 2 |
| Overslung/Underslung | Overslung | Overslung | Overslung |
| Maximum Axle spread (m) | 0.000 | 0.000 | 2.000 |
| Dampers Part Numbers | D8K91-9526W | D8K91-9526W | D8K91-9526W |
| Smallest Tyre Size Designation | 8.25R15 | 8.25R15 | 8.25R15 |
| Highest tyre pressure (Kpa) | 825 | 825 | 825 |
| Airbag Diameter (mm) | 335 | 335 | 335 |
| Reference Drawings No of Suspension (parts list & assembly details) | WE0017314A | WE0018048 | WE0017314A |

|  |  |  |  |
| --- | --- | --- | --- |
|  | Variant 67 | Variant 68 | Variant 69 |
| Variant name: | MBS-200-2 | MBS-100-3 | MBS-200-3 |
| Number of Axles | 2 | 3 | 3 |
| Overslung/Underslung | Overslung | Overslung | Overslung |
| Maximum Axle spread (m) | 2.000 | 3.200 | 3.200 |
| Dampers Part Numbers | D8K91-9526W | D8K91-9526W | D8K91-9526W |
| Smallest Tyre Size Designation | 8.25R15 | 8.25R15 | 8.25R15 |
| Highest tyre pressure (Kpa) | 825 | 825 | 825 |
| Airbag Diameter (mm) | 335 | 335 | 335 |
| Reference Drawings No of Suspension (parts list & assembly details) | WE0018048 | WE0017314A | WE0018048 |

|  |  |  |  |
| --- | --- | --- | --- |
|  | Variant 70 | Variant 71 | Variant 72 |
| Variant name: | WEWELER-HD2 | WEWELER-HD3 | WEWELER-HD4 |
| Number of Axles | 2 | 3 | 4 |
| Overslung/Underslung | U/SLUNG | U/SLUNG | U/SLUNG |
| Maximum Axle spread (m) | 2.000 | 3.200 | 4.900 |
| Dampers Part Numbers | D8K90-2024SP3 | D8K90-2024SP3 | D8K90-2024SP3 |
| Smallest Tyre Size Designation | 8.25R15 | 8.25R15 | 8.25R15 |
| Highest tyre pressure (Kpa) | 825 | 825 | 825 |
| Airbag Diameter (mm) | 350 | 350 | 350 |
| Reference Drawings No of Suspension (parts list & assembly details) | WE0019757 | WE0019757 | WE0019757 |

|  |  |  |  |
| --- | --- | --- | --- |
|  | Variant 73 | Variant 74 | Variant 75 |
| Variant name: | KT230T-2 | KT230T-3 | KI-252T-356-E-F-H |
| Number of Axles | 2 | 3 | 3 |
| Overslung/Underslung | Overslung | Overslung | Overslung |
| Maximum Axle spread (m) | 2.000 | 3.200 | 3.2 |
| Dampers Part Numbers | KONI 912854 | KONI 912854 | N100549-001 |
| Smallest Tyre Size Designation | 8.25R15 | 8.25R15 | 8.25R15 |
| Highest tyre pressure (Kpa) | 825 | 825 | 825 |
| Airbag Diameter (mm) | 335 | 335 | 358-366 |
| Reference Drawings No of Suspension (parts list & assembly details) | N100691-001 | N100691-001 | N100728 |

|  |  |  |  |
| --- | --- | --- | --- |
|  | Variant 76 | Variant 77 | Variant 78 |
| Variant name: | KI-252T-380-E-F-H | KI-252T-406-E-F-H | KI-252T-432-E-F-H |
| Number of Axles | 3 | 3 | 3 |
| Overslung/Underslung | Overslung | Overslung | Overslung |
| Maximum Axle spread (m) | 3.2 | 3.2 | 3.2 |
| Dampers Part Numbers | N100549-001 | N100549-001 | N100549-001 |
| Smallest Tyre Size Designation | 8.25R15 | 8.25R15 | 8.25R15 |
| Highest tyre pressure (Kpa) | 825 | 825 | 825 |
| Airbag Diameter (mm) | 358-366 | 358-366 | 358-366 |
| Reference Drawings No of Suspension (parts list & assembly details) | N100729 | N100730 | N100731 |

|  |  |  |  |
| --- | --- | --- | --- |
|  | Variant 79 | Variant 80 | Variant 81 |
| Variant name: | KI-252T-457-E-F-H | KI-252T-483-E-F-H | KI52U-2A |
| Number of Axles | 3 | 2 | 2 |
| Overslung/Underslung | Overslung | Overslung | Underslung |
| Maximum Axle spread (m) | 3.2 | 2 | 2 |
| Dampers Part Numbers | N100549-001 | N100549-001 | N100549-003 |
| Smallest Tyre Size Designation | 8.25R15 | 8.25R15 | 8.25R15 |
| Highest tyre pressure (Kpa) | 825 | 825 | 825 |
| Airbag Diameter (mm) | 358-366 | 358-366 | 338 |
| Reference Drawings No of Suspension (parts list & assembly details) | N100732 | N100733 | KI252U-FC KI252U-FM KI252U-RC KI252U-RM |

|  |  |  |  |
| --- | --- | --- | --- |
|  | Variant 82 | Variant 83 | Variant 84 |
| Variant name: | KI252U-2B | KI252U-2C | KT230T - 2 |
| Number of Axles | 2 | 2 | 2 |
| Overslung/Underslung | Underslung | Underslung | Overslung |
| Maximum Axle spread (m) | 2 | 2 | 2 |
| Dampers Part Numbers | N100549-004 | WCTA003 | N100549-005 N100549-006 |
| Smallest Tyre Size Designation | 8.25R15 | 8.25R15 | 8.25R15 |
| Highest tyre pressure (Kpa) | 825 | 825 | 825 |
| Airbag Diameter (mm) | 338 | 338 | 335 |
| Reference Drawings No of Suspension (parts list & assembly details) | KI252U-FC KI252U-FM KI252U-RC KI252U-RM | KI252U-FC KI252U-FM KI252U-RC KI252U-RM | N100690 N100691 N100692 N100693 N100694 N100695 N100696 N100697 |

|  |  |  |  |
| --- | --- | --- | --- |
|  | Variant 86 | Variant 87 | Variant 88 |
| Variant name: | KI-252T-432-E-F-H | KI-252T-457-E-F-H | KI252U-1A |
| Number of Axles | 2 | 2 | 1 |
| Overslung/Underslung | Overslung | Overslung | Underslung |
| Maximum Axle spread (m) | 2 | 2 | 1 |
| Dampers Part Numbers | N100549-001 | N100549-001 | N100549-003 |
| Smallest Tyre Size Designation | 8.25R15 | 8.25R15 | 8.25R15 |
| Highest tyre pressure (Kpa) | 825 | 825 | 825 |
| Airbag Diameter (mm) | 358-366 | 358-366 | 338 |
| Reference Drawings No of Suspension (parts list & assembly details) | N100731 | N100732 | KI252U-FC KI252U-FM KI252U-RC KI252U-RM |

|  |  |  |  |
| --- | --- | --- | --- |
|  | Variant 89 | Variant 90 | Variant 91 |
| Variant name: | KI-252T-483-E-F-H | KI252U-3A | KI252U-3B |
| Number of Axles | 3 | 3 | 3 |
| Overslung/Underslung | Overslung | Underslung | Underslung |
| Maximum Axle spread (m) | 3.2 | 3.2 | 3.2 |
| Dampers Part Numbers | N100549-001 | N100549-003 | N100549-004 |
| Smallest Tyre Size Designation | 8.25R15 | 8.25R15 | 8.25R15 |
| Highest tyre pressure (Kpa) | 825 | 825 | 825 |
| Airbag Diameter (mm) | 358-366 | 338 | 338 |
| Reference Drawings No of Suspension (parts list & assembly details) | N100733 | KI252U-FC KI252U-FM KI252U-RC KI252U-RM | KI252U-FC KI252U-FM KI252U-RC KI252U-RM |

|  |  |  |  |
| --- | --- | --- | --- |
|  | Variant 92 | Variant 93 | Variant 94 |
| Variant name: | KI252U-3C | KT230T - 3 |  |
| Number of Axles | 3 | 3 |  |
| Overslung/Underslung | Underslung | Overslung |  |
| Maximum Axle spread (m) | 3.2 | 3.2 |  |
| Dampers Part Numbers | WCTA003 | N100549-005 N100549-006 |  |
| Smallest Tyre Size Designation | 8.25R15 | 8.25R15 |  |
| Highest tyre pressure (Kpa) | 825 | 825 |  |
| Airbag Diameter (mm) | 338 | 335 |  |
| Reference Drawings No of Suspension (parts list & assembly details) | KI252U-FC KI252U-FM KI252U-RC KI252U-RM | N100690 N100691 N100692 N100693 N100694 N100695 N100696 N100697 |  |

…………………………………………….

Umesh Shamdasani

Director

Technical Assessment and Approvals Section

Vehicle Safety Operations Branch

Date: 2 July 2025