**Department of Infrastructure, Transport, Regional Development and Communications**

**Vehicle Safety Operations Branch**

**Road-Friendly Suspension Certificate Number (RFCN): RF2073**

 **Issue Date: 21 February 2022**

The Assistant Secretary, Vehicle Safety Operations Branch, has assessed the information in Schedule 3

for the suspension described in this Road Friendly Certificate, which the Supplier identified in

Schedule 1 has submitted, as complying with the road-friendliness requirements as specified in

NTC publication ‘Road-Friendly Suspension – Performance and Component Requirements, and

Acceptable Test Methods’. This information will be acceptable for use as evidence of compliance

with the requirements specified in the above NTC publication. Provided the suspension is installed

according to the Supplier’s nominated installation instructions identified in Schedule 3.

The issue of this Certificate is subject to the following conditions:

1. The Supplier shall not quote the Road-Friendly Certificate Number in respect of a suspension which is not the suspension certified in the Road–Friendly Suspension certificate with that number.

1. Without the prior approval of the General Manager, Vehicle Safety Standards Branch, the Supplier shall not quote Road-Friendly Certificate Number in respect of a suspension, that is in any way different from the suspension described in the final form of the application for this Suspension Certificate Number. The application includes reports and other information relating to the application.
2. The Supplier shall by detailed quality control and test ensure continuing compliance with the requirements.
3. The Supplier shall maintain records of detailed quality control and test documentation.
4. The Supplier shall supply upon request, to General Manager, Vehicle Safety Standards Branch any additional information requested for the purpose of demonstrating compliance.
5. The Supplier shall not quote the Road-Friendly Certificate Number in respect of a suspension on or after the Expiry date specified in the certificate.
6. The Supplier shall indicate by an appropriate method (decal, label or plate) the Road-Friendly Suspension Certificate Number (RFCN) on the suspension system, or on a suitable location on the vehicle near the installed suspension or the vehicle compliance plate.
7. On cessation of marketing the specified suspension in Australia, the Supplier shall notify General Manager, Vehicle Safety Standards Branch of the date of manufacture of the last specified suspension supplied to the market in Australia.
8. If the requirements for road-friendliness are changed by the National Road Transport Commission, a new approval may be required.

Certificate No: **RF2073**

### Issue Date: 21 February 2022

Expiry Date: **Life of Model**

# SCHEDULE 1

**Supplier Name**: ABS Trailquip Pty Ltd **Supplier ID**:

**Supplier Address**: 150 Beatty Road
ARCHERFIELD QLD 4108

# SCHEDULE 2

**Make:** TRAILQUIP

**Model:** AIR SUSPENSION ROAD FRIENDLY

# SCHEDULE 3

|  |  |  |  |
| --- | --- | --- | --- |
|  | Variant 1 | Variant 2 | Variant 3 |
| Variant name: | TQASA-10-RF-1 | TQASA-20-RF-2 | TQASA-30-RF-3 |
| Number of Axles | 1 | 2 | 3 |
| Overslung/Underslung | Overslung | Overslung | Overslung |
| Maximum Axle spread (m) | 1.000 | 2.000 | 3.200 |
| Dampers Part Numbers | TQA-SA14 | TQA-SA14 | TQA-SA14 |
| Smallest Tyre Size Designation | 8.25R15 | 8.25R15 | 8.25R15 |
| Highest tyre pressure (Kpa) | 825 | 825 | 825 |
| Airbag Diameter (mm) | 250 | 250 | 250 |
| Reference Drawings No of Suspension (parts list & assembly details) | TQASA-30-RF-3 | TQASA-30-RF-3 | TQASA-30-RF-3 |

|  |  |  |  |
| --- | --- | --- | --- |
|  | Variant 4 | Variant 5 | Variant 6 |
| Variant name: | TQASA-40-SP-4 | TQASA-30-SP-3 | TQASA-20-SP-2 |
| Number of Axles | 4 | 3 | 2 |
| Overslung/Underslung | Overslung | Overslung | Overslung |
| Maximum Axle spread (m) | 4.900 | 3.200 | 2.000 |
| Dampers Part Numbers | TQA-SA25 | TQA-SA25 | TQA-SA25 |
| Smallest Tyre Size Designation | 8.25R15 | 8.25R15 | 8.25R15 |
| Highest tyre pressure (Kpa) | 825 | 825 | 825 |
| Airbag Diameter (mm) | 340 | 340 | 340 |
| Reference Drawings No of Suspension (parts list & assembly details) | TQASA-20-SP-2 | TQASA-20-SP-2 | TQASA-20-SP-2 |

|  |  |  |  |
| --- | --- | --- | --- |
|  | Variant 7 | Variant 8 | Variant 9 |
| Variant name: | TQA-SFDOL-360-1 | TQA-SFDOL-360-2 | TQA-SFDOL-360-3 |
| Number of Axles | 1 | 2 | 3 |
| Overslung/Underslung | U/Slung | U/Slung | U/Slung |
| Maximum Axle spread (m) | 0.000 | 2.000 | 3.200 |
| Dampers Part Numbers | TQA-SA45 | TQA-SA45 | TQA-SA45 |
| Smallest Tyre Size Designation | 265/75R19.5 | 265/75R19.5 | 265/75R19.5 |
| Highest tyre pressure (Kpa) | 825 | 825 | 825 |
| Airbag Diameter (mm) | 266 | 266 | 266 |
| Reference Drawings No of Suspension (parts list & assembly details) | TQA-SFDOL-360-1 | TQA-SFDOL-360-1 | TQA-SFDOL-360-1 |

…………………………………………….

Umesh Shamdasani

Director of Technical Assessment and Approvals team

Vehicle Safety Operations Branch

 February 2022